April 30, 2024

SUPPLEMENTAL BULLETIN NO. 1

SUBJECT: Corrigendum to Section VII. Technical Specifications

This Supplemental Bulletin is issued to amend provisions in the Bidding Documents (BDs) for the project “*Supply, Delivery, Installation and Maintenance of ICT Equipment and Network Improvement Project of DepEd Regional Office IX - DCP FY 2023* ”.

|  |  |  |
| --- | --- | --- |
| **Item** | **Specification** | **Statement of Compliance** |
| 1 | **One (1) Unit**  **High-performance data management solution Rack Station** Server with up to 36-bay, 6 core 2.2 GHz base and 2.7 GHz turbo processor speed, 5 years warranty, 32GB RAM, and 96TB NAS Drives SATA 7200RPM 6Gbps, 10Gbe NIC Support, Redundant Power  - With Rail Kit Sliding |  |
| 2 | **One (1) Unit**  **Network Remote and Live Streaming Notebook** with Intel Core Ultra 7 Processor (2024), NVIDIA GeForce RTX 4070 Laptop GPU (8GB), Nebula OLED 16-inch 2.5K (2560x1600) 16:10 aspect ration display, 32GB LPDDR5X 7467 Memory, 2TB PCIE 4.0 NVME M.2 SSD, Ports (3.5mm Combo Audio Jack, HDMI 2.1, USB 3.2 Gen 1-Type A and Gen 2-Type C, RJ45 Lan Port, Thunderbolt 4 Support Display Port, Card Reader (SD)), Backlit Chiclet Keyboard 1-Zone RGB, Touchpad, 1080P FHD IR Camera for Windows Hello, Wifi 6E, 90WHrs 4S1 4 Cell Lion Battery, Power Supply a.)(Rectangle Conn, 200W AC Adapter, Output 20V, Input 100-240V) b.) (Type C, 100W AC Adapter, Output: 20V DC, Input: 100-240V AC), Slash Lighting, Preferred Color (White), G16 Sleeve, Impact Mouse |  |
| 3 | **One (1) Unit**  **RF 200-800mm F6.3-9 IS, Mounts on Full-Frame, APS-C**  - USM Aperture Range - Wide / Long f/6.3-32 / f/9.0-54 |  |
| 4 | **One (1) Unit**  **AIO | 27inch FHD | Core i7-1260P Processor | 8GB RAM | 256GB SSD + 1TB HDD Storage| 2GB NVIDIA Video Card**  - Integrated 5.0 MP Full HD Camera, - Wifi and Bluetooth  - Display: 27 inch display, - Ports: LAN Gigabit Ethernet, HDMI Port, USB 3.1, USB Type C Port, - Wireless Keyboard and Mouse |  |
| 5 | **One (1) Piece**  **1 PC 32 CHANNEL ULTRA 4K H.265 NETWORK VIDEO RECORDER (NVR) + 4PC 8MP Lite IR Fixed-focal Dome Network Camera 12V DC/PoE power supply + 4 PC 8MP Lite IR Vari-focal Bullet Network Camera 12V DC/PoE power supply**  - Video Outputs: 2 pcs HMI, 1 pcs VGA, - Network Protocols: HTTP, TCP/IP, IPv4/IPv6, UPNP, DHCP, - Intel Processor, - 2x 6TB Surveillance Grade Storage |  |
| 6 | **Three (3) Pieces**  **28-Port Gigabit Smart Switch with 24-Port PoE+**  - 24× 10/100/1000 Mbps RJ45 Ports (Auto Negotiation/Auto MDI/MDIX), - 4× Gigabit SFP Slots, - VLAN: VLAN Group Max. 4K VLAN |  |

This Supplemental Bulletin shall form an integral part of the said Bidding Documents.

For the guidance and information of all concerned.

(SGD) **DR. GREGORIO CYRUS R. ELEJORDE, CESO V**

Assistant Regional Director

Chairperson, Bids and Awards Committee